

**Australian Government Building and Construction WHS Accreditation Scheme**

**Analysis of Biannual Data from Accredited Contractors**

**July to December 2015**

**Reporting Period**



Contents

[1 Introduction 3](#_Toc444846214)

[2 Overview 3](#_Toc444846215)

[2.1 Number of Accredited contractors 3](#_Toc444846216)

[2.2 Applications 4](#_Toc444846217)

[2.3 Number of Projects 5](#_Toc444846218)

[3 Analysis/Findings 7](#_Toc444846219)

[3.1 Fatalities 7](#_Toc444846220)

[3.2 Lost Time Injury Frequency Rate (LTIFR) 8](#_Toc444846221)

[3.3 Medically Treated Injury Frequency Rate (MTIFR) 10](#_Toc444846222)

[3.4 Total Recorded Injury Frequency Rate (TRIFR) 11](#_Toc444846223)

[3.5 LTIFR/MTIFR/TRIFR Summary 12](#_Toc444846224)

[3.6 Number of Notices Issued 14](#_Toc444846225)

[4 Incidents 15](#_Toc444846226)

[4.1 Nature of Injury 15](#_Toc444846227)

[4.2 Mechanism of Injury 16](#_Toc444846228)

[4.3 Location of Injury 17](#_Toc444846229)

[4.4 High-risk Construction Work 19](#_Toc444846230)

[4.5 Working Time Lost 22](#_Toc444846231)

[4.6 Age Breakdown 23](#_Toc444846232)

[4.7 Injured Person’s Occupation 24](#_Toc444846233)

[4.8 Dangerous Occurrences 25](#_Toc444846234)

[4.9 Workers’ Compensation 26](#_Toc444846235)

[5 Awards and Recognition 27](#_Toc444846236)

[6 Initiatives 27](#_Toc444846237)

[Glossary 28](#_Toc444846238)8

# 1 Introduction

This report is produced by the Office of the Federal Safety Commissioner (OFSC). The report provides an overview and analysis of data collected from companies accredited under the Australian Government Building and Construction WHS Accreditation Scheme (the Scheme) for the period July to December 2015. Comparisons are also made with data collected from previous biannual periods where appropriate.

Under their conditions of accreditation, accredited contractors are required to submit biannual reports twice a year, in addition to incident reports, Scheme project reports and end of project reports. The data used in this report has been collected from a combination of biannual, incident and Scheme project reports.

Key terms and performance measures used throughout this report are defined in the Glossary commencing on page 28.

# 2 Overview

## 2.1 Number of Accredited Contractors

The number of accredited contractors continues to grow, with 331[[1]](#footnote-1) contractors submitting biannual reports for the July to December 2015 reporting period. This is a 4.42 per cent increase on the previous period. The number of accredited contractors has increased every year since the Scheme commenced in 2006. Of the 331 accredited contractors, 202 (61.03 per cent) did not undertake Scheme projects during the period, with 33 (9.97 per cent) undertaking no projects as the head contractor during the period.

## 2.2 Applications and Accreditations

The OFSC continues to receive new applications from companies seeking accreditation under the Scheme with 39 applications for initial accreditation received during the July to December 2015 reporting period.

Forty-seven reaccreditation applications were received during the period, bringing the total number of applications to 86, which is an increase compared to the previous corresponding period (79 total for July to December 2014). Twenty-three contractors gained accreditation for the first time during the period, while 43 contractors achieved reaccreditation.

| Period | Applications for First Accreditation | Applications for Reaccreditation | Total Applications |
| --- | --- | --- | --- |
| 2006 | 24 | 0 | 24 |
| Jan to Jun 2007 | 61 | 0 | 61 |
| Jul to Dec 2007 | 50 | 0 | 50 |
| Jan to Jun 2008 | 35 | 0 | 35 |
| Jul to Dec 2008 | 41 | 0 | 41 |
| Jan to Jun 2009 | 58 | 0 | 58 |
| Jul to Dec 2009 | 48 | 17 | 65 |
| Jan to Jun 2010 | 29 | 34 | 63 |
| July to Dec 2010 | 39 | 30 | 69 |
| Jan to Jun 2011 | 34 | 19 | 53 |
| Jul to Dec 2011 | 38 | 26 | 64 |
| Jan to Jun 2012 | 33 | 19 | 52 |
| Jul to Dec 2012 | 27 | 37 | 64 |
| Jan to Jun 2013 | 41 | 36 | 77 |
| Jul to Dec 2013 | 48 | 32 | 80 |
| Jan to Jun 2014 | 45 | 36 | 81 |
| Jul to Dec 2014 | 46 | 33 | 79 |
| Jan to Jun 2015 | 35 | 24 | 59 |
| Jul to Dec 2015 | 39 | 47 | 86 |
| Total | 771 | 390 | 1,161 |

## 2.3 Number of Projects and Hours Worked

The OFSC has been notified of a total of 1429 directly and indirectly funded contracts for building work with a combined value of $84.24 billion that had been covered by the Scheme (as at 31 December 2015). Of the 1429 notified contracts, 289 were active and 1140 were completed at the end of this reporting period.

The data gathered for this current reporting period includes non-Scheme projects valued at less than $3 million. The data prior to the July 2010 reporting period only includes projects with a value of $3 million or more.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Period | Number of Accredited contractors reporting active Scheme projects | Number of active Scheme Projects | Number of Accredited contractors reporting non-Scheme projects | Number of non-Scheme projects where accredited contractor was the head contractor |
| Jul to Dec 2007 | 25 | 42 | 58 | 1,019 |
| Jan to Jun 2008 | 32 | 71 | 85 | 1,212 |
| Jul to Dec 2008 | 44 | 103 | 107 | 1,416 |
| Jan to Jun 2009 | 61 | 128 | 124 | 1,730 |
| Jul to Dec 2009 | 75 | 183 | 145 | 2,170 |
| Jan to Jun 2010 | 94 | 249 | 153 | 2,255 |
| Jul to Dec 2010 | 102 | 293 | 177 | 6,943 |
| Jan to Jun 2011 | 108 | 329 | 185 | 7,861 |
| Jul to Dec 2011 | 113 | 343 | 197 | 11,081 |
| Jan to Jun 2012 | 110 | 357 | 218 | 8,824 |
| Jul to Dec 2012 | 117 | 347 | 228 | 7,235 |
| Jan to Jun 2013 | 126 | 339 | 237 | 11,568 |
| Jul to Dec 2013 | 137 | 362 | 254 | 13,016 |
| Jan to Jun 2014 | 136 | 335 | 269 | 13,700 |
| Jul to Dec 2014 | 129 | 306 | 277 | 13,328 |
| Jan to Jun 2015 | 128 | 295 | 288 | 13,772 |
| Jul to Dec 2015 | 129 | 289 | 298 | 9,164 |

Hours worked on Scheme and Non-Scheme projects

|  |  |  |  |
| --- | --- | --- | --- |
| Period | Scheme projects  (million hours) | Non-Scheme projects  any value  (million hours) | All projects  (million hours) |
| Jul to Dec 2010 | 41.97 | 147.44 | 189.40 |
| Jan to Jun 2011 | 26.29 | 135.95 | 162.24 |
| Jul to Dec 2011 | 31.92 | 135.29 | 167.20 |
| Jan to Jun 2012 | 29.94 | 139.57 | 169.51 |
| Jul to Dec 2012 | 43.80 | 131.05 | 174.85 |
| Jan to Jun 2013 | 33.66 | 135.78 | 169.45 |
| Jul to Dec 2013 | 31.86 | 152.89 | 184.75 |
| Jan to Jun 2014 | 30.57 | 137.86 | 168.44 |
| Jul to Dec 2014 | 30.06 | 151.78 | 181.84 |
| Jan to Jun 2015 | 27.41 | 149.31 | 176.71 |
| Jul to Dec 2015 | 26.14 | 146.37 | 172.51 |

# 3 Analysis/Findings

## 3.1 Fatalities

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Period | Number of Fatalities on Scheme projects | Scheme project Fatalities frequency rate | Number of Fatalities on non-Scheme projects | Non-Scheme projects Fatalities frequency rate | Number of Fatalities all projects | All projects Fatalities frequency rate |
| Jul to Dec 2007 | 1 | NA | 0 | NA | 1 | NA |
| Jan to Jun 2008 | 0 | NA | 6 | NA | 6 | NA |
| Jul to Dec 2008 | 0 | NA | 4 | NA | 4 | NA |
| Jan to Jun 2009 | 1 | NA | 4 | NA | 5 | NA |
| Jul to Dec 2009 | 0 | 0.00 | 1 | 1.07 | 1 | 0.92 |
| Jan to Jun 2010 | 1 | 4.36 | 0 | 0.00 | 1 | 0.66 |
| Jul to Dec 2010 | 2 | 4.77 | 2 | 1.35 | 4 | 2.39 |
| Jan to Jun 2011 | 0 | 0.00 | 1 | 0.70 | 1 | 0.60 |
| Jul to Dec 2011 | 3 | 9.40 | 3 | 2.22 | 6 | 3.59 |
| Jan to Jun 2012 | 0 | 0.00 | 6 | 4.85 | 6 | 3.90 |
| Jul to Dec 2012 | 2 | 4.57 | 3 | 2.29 | 5 | 2.86 |
| Jan to Jun 2013 | 2 | 5.94 | 3 | 2.21 | 5 | 2.95 |
| Jul to Dec 2013 | 0 | 0.00 | 1 | 0.66 | 1 | 0.54 |
| Jan to Jun 2014 | 0 | 0.00 | 0 | 0.00 | 0 | 0.00 |
| Jul to Dec 2014 | 0 | 0.00 | 2 | 1.32 | 2 | 1.10 |
| Jan to Jun 2015 | 0 | 0.00 | 1 | 0.67 | 1 | 0.57 |
| Jul to Dec 2015 | 0 | 0.00 | 2 | 1.37 | 2 | 1.16 |

## 3.2 Lost Time Injury Frequency Rate (LTIFR)

The OFSC began monitoring the LTIFR for Scheme and non-Scheme projects in the July to December 2007 reporting period. Since then there has been an average 54.99 per cent decrease in the Scheme project Winsorised mean LTIFR and an average 41.59 per cent decrease in the non‑Scheme project Winsorised mean LTIFR when comparing each of the previous reporting periods to the current period. For this period, the Scheme project Winsorised mean LTIFR was 48.08 per cent lower than the non-Scheme project Winsorised mean LTIFR.

There has been a 78.26 per cent decrease in the Scheme project Winsorised mean LTIFR when comparing the current period to the corresponding period in 2008. Individual company data shows that the LTIFR decreases significantly the longer a company retains accreditation under the scheme. After 6 years of accreditation, 72 per cent of companies have reduced their LTIFR by an average of 77 per cent.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Period | Scheme project median | Scheme project Arithmetic mean | Scheme project Winsorised mean | Non-Scheme project median | Non-Scheme project Arithmetic mean | Non-Scheme Project Winsorised mean |
| Jul to Dec 2007 | 0.00 | 6.94 | 4.04 | 4.65 | 10.06 | 7.52 |
| Jan to Jun 2008 | 0.00 | 9.24 | 8.72 | 4.95 | 10.41 | 9.05 |
| Jul to Dec 2008 | 0.00 | 7.44 | 6.21 | 4.65 | 12.22 | 7.36 |
| Jan to Jun 2009 | 0.00 | 12.86 | 10.35 | 3.50 | 11.54 | 6.10 |
| Jul to Dec 2009 | 0.00 | 9.36 | 7.68 | 3.00 | 11.61 | 8.28 |
| Jan to Jun 2010 | 0.00 | 21.99 | 3.21 | 3.73 | 11.34 | 8.61 |
| Jul to Dec 2010 | 0.00 | 5.54 | 3.43 | 0.00 | 13.83 | 4.76 |
| Jan to Jun 2011 | 0.00 | 10.17 | 3.98 | 0.00 | 8.97 | 3.97 |
| Jul to Dec 2011 | 0.00 | 20.60 | 6.82 | 0.60 | 8.01 | 5.45 |
| Jan to Jun 2012 | 0.00 | 4.14 | 2.04 | 0.00 | 7.38 | 4.30 |
| Jul to Dec 2012 | 0.00 | 13.54 | 1.88 | 0.00 | 6.15 | 2.71 |
| Jan to Jun 2013 | 0.00 | 6.10 | 1.69 | 0.00 | 21.60 | 3.87 |
| Jul to Dec 2013 | 0.00 | 8.88 | 3.93 | 0.00 | 7.69 | 3.13 |
| Jan to Jun 2014 | 0.00 | 11.03 | 1.40 | 0.00 | 7.42 | 3.88 |
| Jul to Dec 2014 | 0.00 | 4.61 | 2.56 | 0.00 | 5.47 | 2.78 |
| Jan to Jun 2015 | 0.00 | 3.37 | 1.64 | 0.00 | 4.64 | 2.69 |
| Jul to Dec 2015 | 0.00 | 7.30 | 1.35 | 0.00 | 5.49 | 2.60 |

**Scheme LTIFR by construction type**

When separated by industry sector, Scheme work carried out by accredited contractors on Residential projects recorded the highest mean LTIFR (41.03), followed by Civil projects (3.93) and Commercial projects (3.75). The arithmetic mean LTIFR for Residential was significantly higher than other construction types due to a smaller sample size and one outlier. The Winsorised mean is a more accurate reflection of the LTIFR for the period.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Residential | Civil | Commercial | All |
| Mean | 41.03 | 3.93 | 3.75 | 7.30 |
| Median | 0.00 | 0.00 | 0.00 | 0.00 |
| Winsorised Mean | 1.09 | 0.46 | 1.51 | 1.35 |

**Non-Scheme LTIFR by construction type**

Non-Scheme work carried out by accredited contractors on Commercial projects recorded the highest mean LTIFR (7.24), followed by Civil projects (4.81) and Residential projects (4.16).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Residential | Civil | Commercial | All |
| Mean | 4.16 | 4.81 | 7.24 | 5.49 |
| Median | 0.00 | 0.00 | 0.00 | 0.00 |
| Winsorised Mean | 0.98 | 0.79 | 3.62 | 2.60 |

## 

## 3.3 Medically Treated Injury Frequency Rate (MTIFR)

When comparing each of the previous reporting periods to the current period, there has been an average 31.60 per cent decrease in the Scheme project Winsorised mean MTIFR and an average 20.32 per cent decrease in the non-Scheme project MTIFR Winsorised.

The MTIFR for Scheme projects is consistently significantly lower than the MTIFR for non-Scheme projects; the average difference since July 2007 is 52.84 per cent when comparing the Winsorised mean.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Period | Scheme project median | Scheme project Arithmetic mean | Scheme project Winsorised mean | Non-Scheme project median | Non-Scheme project Arithmetic mean | Non-Scheme Project Winsorised mean |
| Jul to Dec 2007 | 0.00 | 12.06 | 9.53 | 19.90 | 26.23 | 23.32 |
| Jan to Jun 2008 | 0.00 | 18.06 | 16.29 | 19.00 | 29.39 | 24.36 |
| Jul to Dec 2008 | 2.78 | 21.79 | 14.50 | 13.18 | 21.10 | 16.67 |
| Jan to Jun 2009 | 8.58 | 33.93 | 22.78 | 14.32 | 26.82 | 17.21 |
| Jul to Dec 2009 | 13.04 | 21.84 | 16.62 | 18.17 | 38.51 | 28.73 |
| Jan to Jun 2010 | 0.00 | 34.67 | 16.95 | 21.03 | 40.15 | 28.45 |
| Jul to Dec 2010 | 0.00 | 11.30 | 6.44 | 12.71 | 63.91 | 21.07 |
| Jan to Jun 2011 | 0.00 | 19.93 | 8.12 | 11.02 | 36.31 | 20.00 |
| Jul to Dec 2011 | 0.00 | 16.30 | 7.23 | 10.83 | 34.12 | 18.10 |
| Jan to Jun 2012 | 0.00 | 13.13 | 9.65 | 10.24 | 32.21 | 18.69 |
| Jul to Dec 2012 | 0.00 | 14.77 | 5.00 | 9.08 | 40.91 | 17.16 |
| Jan to Jun 2013 | 0.00 | 7.52 | 3.78 | 8.28 | 29.95 | 16.89 |
| Jul to Dec 2013 | 0.00 | 11.96 | 5.52 | 8.36 | 52.12 | 16.90 |
| Jan to Jun 2014 | 0.00 | 6.58 | 4.47 | 7.22 | 22.02 | 14.44 |
| Jul to Dec 2014 | 0.00 | 7.95 | 3.95 | 5.60 | 34.36 | 15.32 |
| Jan to Jun 2015 | 0.00 | 7.47 | 3.81 | 5.27 | 22.43 | 14.48 |
| Jul to Dec 2015 | 0.00 | 10.44 | 3.83 | 4.11 | 24.55 | 14.10 |

**Scheme MTIFR by construction type**

Scheme Commercial projects recorded the highest mean MTIFR (14.26), followed by Civil projects (8.31) and Residential projects (3.45). The winsorised mean MTIFR for all construction types were significantly lower than their arithmetic mean; the result of a number of high outliers.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Residential | Civil | Commercial | All |
| Mean | 3.45 | 8.31 | 14.26 | 10.44 |
| Median | 0.00 | 0.00 | 0.00 | 0.00 |
| Winsorised Mean | 0.00 | 1.94 | 7.48 | 3.83 |

**Non-Scheme MTIFR by construction type**

Non-Scheme Commercial projects recorded the highest mean MTIFR (33.99), followed by Civil projects (14.32) and Residential projects (10.75). The winsorised mean MTIFR for Commercial and Civil construction were significantly lower than their arithmetic means; the result of a number of high outliers.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Residential | Civil | Commercial | All |
| Mean | 10.75 | 14.32 | 33.99 | 24.55 |
| Median | 0.00 | 0.00 | 10.26 | 4.11 |
| Winsorised Mean | 8.95 | 7.97 | 18.71 | 14.10 |

## 3.4 Total Recorded Injury Frequency Rate (TRIFR)

In response to industry feedback the OFSC has included a Total Recorded Injury Frequency Rate (TRIFR) calculation to the biannual data analysis report, commencing from the January to June 2014 biannual period onwards.

***Note: TRIFR does not include hours worked on projects less than $3 million, or fatalities on projects less than $3 million.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Period | Scheme project median | Scheme project Arithmetic mean | Scheme project Winsorised mean | Non-Scheme project median | Non-Scheme project Arithmetic mean | Non-Scheme Project Winsorised mean |
| Jan to Jun 2014 | 0.00 | 17.61 | 8.04 | 12.05 | 29.44 | 20.65 |
| Jul to Dec 2014 | 0.00 | 12.56 | 7.40 | 10.07 | 39.83 | 20.44 |
| Jan to Jun 2015 | 0.00 | 10.84 | 6.89 | 8.23 | 27.09 | 18.58 |
| Jul to Dec 2015 | 0.00 | 17.74 | 8.25 | 7.18 | 30.05 | 18.32 |

**Scheme TRIFR by construction type**

Scheme Residential construction projects recorded the highest mean TRIFR (44.48), followed by Commercial projects (18.02) and Civil projects (12.24). As with LTIFR, the arithmetic mean TRIFR for Residential was significantly higher than other construction types due to a smaller sample size and one outlier. The Winsorised mean is a more accurate reflection of the TRIFR for the period.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Residential | Civil | Commercial | All |
| Mean | 44.48 | 12.24 | 18.02 | 17.74 |
| Median | 0.00 | 0.00 | 0.00 | 0.00 |
| Winsorised Mean | 5.39 | 4.91 | 12.03 | 8.25 |

**Non-Scheme TRIFR by construction type**

Non-Scheme Commercial projects recorded the highest mean TRIFR (41.23), followed by Civil projects (20.00) and Residential projects (14.91).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Residential | Civil | Commercial | All |
| Mean | 14.91 | 20.00 | 41.23 | 30.05 |
| Median | 0.00 | 1.84 | 13.17 | 7.18 |
| Winsorised Mean | 10.79 | 12.67 | 23.86 | 18.32 |

## 3.5 LTIFR/MTIFR/TRIFR Summary

The graph below summarises the LTIFR figures across construction types and Scheme and non-Scheme projects. The Scheme LTIFR exceeds the non-Scheme LTIFR on Residential and All projects whereas the non-Scheme LTIFR exceeds the Scheme LTIFR on Commercial and Civil projects.

The following graph summarises the MTIFR figures across construction types and Scheme and non-Scheme projects, with the Scheme MTIFR never exceeding the non-Scheme MTIFR.

The following graph summarises the TRIFR figures across construction types and Scheme and non-Scheme projects, with the non-Scheme TRIFR exceeding the Scheme TRIFR in Commercial, Civil and All projects. The Scheme TRIFR exceeded the non-Scheme TFIFR in Residential projects.

## 3.6 Number of Notices Issued

Part E of the Biannual Report records the outcomes of work cover assessments or court actions issued by the relevant WHS authority of the jurisdiction in which the project is being undertaken. Accredited contractors report the number of notices issued to them as the head contractor or subcontractor, and notices issued to their subcontractors working on site during the period. The types of notices are:

**Infringement**

WHS regulations may allow for infringement notices to be issued as an alternative to prosecution for an offence that is not indictable.

**Prohibition**

Prohibition notices are issued for any work that involves or will involve an immediate risk to the health, safety and welfare of any person.

**Improvement**

Issued if the WHS authority believes someone has contravened the Act or regulations of the jurisdiction, or that a contravention may continue to be repeated. An improvement notice may also include directions about how to remedy a breach.

**Other – (e.g. enforceable undertakings)**

A WHS related notice (other than an infringement, prohibition or improvement notice) issued by the relevant WHS authority in the jurisdiction in which the project is being undertaken.

There has been a significant decrease (54.39 per cent) in the number of Improvement notices issued to accredited contractors when compared to the corresponding period in 2014. The total notices (73) for the January to June 2015 period is the lowest total number of notices reported in the history of the Scheme.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Period | Infringement Notices | Prohibition Notices | Improvement Notices | Other Notices (e.g. enforceable undertakings) | Total Notices |
| Jan to Jun 2011 | 10 | 63 | 140 | 7 | 220 |
| Jul to Dec 2011 | 2 | 51 | 137 | 1 | 191 |
| Jan to Jun 2012 | 4 | 52 | 136 | 5 | 197 |
| Jul to Dec 2012 | 46 | 46 | 143 | 5 | 240 |
| Jan to Jun 2013 | 8 | 41 | 112 | 5 | 166 |
| Jul to Dec 2013 | 1 | 43 | 104 | 7 | 155 |
| Jan to Jun 2014 | 5 | 39 | 126 | 3 | 173 |
| Jul to Dec 2014 | 0 | 35 | 114 | 4 | 153 |
| Jan to Jun 2015 | 0 | 24 | 43 | 7 | 74 |
| Jul to Dec 2015 | 0 | 10 | 52 | 11 | 73 |

# 4 Incidents

Accredited contractors are required to provide incident reports for lost time injuries, medically treated injuries and notifiable dangerous occurrences that occur on Scheme projects, as well as lost time injuries that occur on non-Scheme projects valued at greater than $3 million. Incident reports for all fatalities—regardless of project value—must also be submitted.

## 4.1 Nature of Injury

*Wounds, lacerations, amputations and internal organ damage* injuries (39.62 per cent) have slightly decreased when compared to the corresponding period in 2014, but still remain the highest occurring injuries, while 29.83 per cent of injuries relate to *Traumatic joint/ligament and muscle/tendons*. These two categories make up two thirds of the total injuries reported.

Since the January to June 2012 reporting period, *Wounds, lacerations, amputations and internal organ damage* injuries and *Traumatic joint/ligament and muscle/tendons* have been the first and second most reported injury category respectively.

**Nature of Injury**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Period | Injury A | Injury B | Injury C | Injury D | Injury E | Injury F | Injury G | Injury H |
| Jul to Dec 2011 | 0.76% | 10.51% | 32.57% | 1.43% | 1.24% | 33.81% | 19.20% | 0.48% |
| Jan to Jun 2012 | 0.87% | 9.89% | 38.57% | 1.24% | 1.11% | 31.77% | 15.70% | 0.87% |
| Jul to Dec 2012 | 0.81% | 12.53% | 37.06% | 2.02% | 1.62% | 26.95% | 17.65% | 1.35% |
| Jan to Jun 2013 | 0.16% | 12.28% | 43.22% | 2.71% | 0.48% | 21.69% | 19.14% | 0.32% |
| Jul to Dec 2013 | 0.78% | 13.40% | 36.92% | 2.49% | 0.93% | 28.97% | 14.95% | 1.56% |
| Jan to Jun 2014 | 0.18% | 15.64% | 39.54% | 0.70% | 1.05% | 26.89% | 15.29% | 0.70% |
| Jul to Dec 2014 | 0.74% | 13.84% | 36.72% | 0.55% | 0.37% | 31.18% | 16.24% | 0.37% |
| Jan to Jun 2015 | 0.21% | 15.00% | 38.96% | 2.29% | 0.63% | 29.58% | 13.33% | 0.00% |
| Jul to Dec 2015 | 0.48% | 14.80% | 39.62% | 1.19% | 0.48% | 29.83% | 13.60% | 0.00% |

## 4.2 Mechanism of Injury

The top four mechanisms of injury reported to the OFSC were *Falls, trips and slips of a person* (27.45 per cent), *Being hit by moving objects* (25.78 per cent), *Hitting objects with part of the body* (23.63 per cent) and *Body Stressing* (15.75 per cent). These mechanisms account for 92.61 per cent of all injuries reported during the period. These are the same four categories that were the top four identified in the corresponding period for the previous year.

**Mechanism of Injury**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Period | Mech. 0 | Mech. 1 | Mech. 2 | Mech. 3 | Mech. 4 | Mech. 5 | Mech. 6 | Mech. 7 | Mech. 8 | Mech. 9 |
| Jul to Dec 2011 | 20.92% | 21.78% | 23.78% | 0.29% | 24.74% | 2.10% | 1.91% | 0.67% | 0.00% | 3.82% |
| Jan to Jun 2012 | 21.26% | 23.49% | 25.34% | 0.00% | 20.64% | 2.84% | 2.10% | 1.73% | 0.25% | 2.35% |
| Jul to Dec 2012 | 21.83% | 20.89% | 28.57% | 0.13% | 19.54% | 3.91% | 1.62% | 0.94% | 0.27% | 2.29% |
| Jan to Jun 2013 | 15.31% | 24.40% | 31.74% | 1.12% | 17.38% | 4.15% | 2.71% | 0.32% | 0.16% | 2.71% |
| Jul to Dec 2013 | 19.00% | 19.78% | 28.97% | 0.62% | 22.90% | 2.65% | 2.02% | 0.62% | 0.00% | 3.43% |
| Jan to Jun 2014 | 23.20% | 25.31% | 26.36% | 0.18% | 18.45% | 1.41% | 0.88% | 0.88% | 0.00% | 3.34% |
| Jul to Dec 2014 | 26.94% | 18.82% | 30.26% | 0.18% | 16.61% | 1.66% | 2.21% | 0.92% | 0.00% | 2.40% |
| Jan to Jun 2015 | 25.36% | 22.45% | 28.07% | 0.21% | 16.01% | 2.49% | 1.46% | 1.04% | 0.42% | 2.49% |
| Jul to Dec 2015 | 27.45% | 23.63% | 25.78% | 0.00% | 15.75% | 1.67% | 2.15% | 0.24% | 0.24% | 3.10% |

## 4.3 Location of Injury

Almost 70 per cent of injuries reported were sustained to *upper limbs* (41.29 per cent) and *lower limbs* (28.64 per cent).

**Location of Injury**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Period | Loc. 1 | Loc. 2 | Loc. 3 | Loc. 4 | Loc. 5 | Loc. 6 | Loc. 7 | Loc. 8 | Loc. 9 |
| Jul to Dec 2011 | 10.51% | 1.81% | 20.92% | 34.48% | 27.22% | 2.29% | 0.29% | 0.19% | 2.29% |
| Jan to Jun 2012 | 9.52% | 2.10% | 16.81% | 37.33% | 28.55% | 2.10% | 0.25% | 0.62% | 2.72% |
| Jul to Dec 2012 | 11.19% | 1.21% | 17.12% | 34.91% | 27.49% | 3.50% | 0.27% | 0.27% | 4.04% |
| Jan to Jun 2013 | 12.12% | 1.12% | 14.83% | 36.84% | 28.71% | 2.55% | 0.32% | 0.64% | 2.87% |
| Jul to Dec 2013 | 10.44% | 1.25% | 13.86% | 40.65% | 28.19% | 3.58% | 0.47% | 0.31% | 1.25% |
| Jan to Jun 2014 | 8.44% | 2.64% | 15.11% | 38.84% | 30.58% | 1.76% | 0.88% | 0.18% | 1.58% |
| Jul to Dec 2014 | 8.49% | 2.03% | 16.61% | 38.56% | 29.52% | 1.66% | 0.92% | 0.00% | 2.21% |
| Jan to Jun 2015 | 8.73% | 1.87% | 13.51% | 40.75% | 30.98% | 2.29% | 0.00% | 0.62% | 1.25% |
| Jul to Dec 2015 | 9.79% | 1.67% | 14.56% | 41.29% | 28.64% | 3.10% | 0.24% | 0.24% | 0.48% |

## 

## 4.4 High-risk Construction Work

When submitting incident reports, accredited contractors are required to disclose – where applicable – what was the most significant high-risk construction work taking place at the time of the incident. Of the incident reports submitted, 40.91 per cent nominated high-risk construction work as having been undertaken at the time of the incident. The three most common categories of high-risk work taking place at the time of an incident were:

* construction work on construction sites where there is any movement of powered mobile plant (40.00 per cent)
* construction work with risk of a person falling two metres or more (20.00 per cent)
* construction work on or near energised electrical installations and services (14.07 per cent)

\*See glossary for high-risk construction work details.

**High-risk Construction Work**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Period | Jul to Dec 2011 | Jan to Jun 2012 | Jul to Dec 2012 | Jan to Jun 2013 | Jul to Dec 2013 | Jan to Jun 2014 | Jul to Dec 2014 | Jan to Jun 2015 | Jul to Dec 2015 |
| Risk 1 | 20.81% | 16.73% | 16.46% | 11.63% | 13.68% | 17.90% | 16.95% | 15.65% | 20.00% |
| Risk 2 | 0.00% | 0.00% | 0.41% | 0.00% | 0.00% | 1.23% | 0.56% | 0.68% | 2.96% |
| Risk 3 | 2.54% | 4.67% | 1.65% | 2.33% | 3.16% | 3.70% | 3.95% | 2.04% | 2.96% |
| Risk 4 | 0.00% | 1.56% | 0.82% | 1.86% | 3.16% | 3.70% | 0.56% | 6.12% | 1.48% |
| Risk 5 | 2.03% | 1.95% | 2.06% | 2.33% | 2.11% | 5.56% | 9.04% | 6.12% | 5.93% |
| Risk 6 | 0.00% | 1.17% | 0.82% | 0.00% | 0.53% | 0.62% | 0.00% | 0.00% | 0.00% |
| Risk 7 | 2.54% | 1.95% | 2.47% | 3.26% | 3.68% | 1.85% | 2.26% | 0.68% | 2.22% |
| Risk 8 | 0.51% | 1.95% | 7.00% | 5.58% | 3.16% | 6.79% | 3.95% | 5.44% | 0.74% |
| Risk 9 | 0.00% | 0.39% | 0.41% | 0.00% | 0.00% | 0.00% | 0.00% | 0.00% | 0.00% |
| Risk 10 | 0.00% | 1.56% | 0.00% | 3.72% | 2.63% | 4.94% | 0.56% | 3.40% | 1.48% |
| Risk 11 | 0.51% | 1.56% | 0.00% | 0.00% | 0.00% | 0.00% | 0.00% | 1.36% | 0.74% |
| Risk 12 | 2.54% | 8.56% | 8.23% | 13.02% | 10.00% | 4.32% | 9.04% | 10.20% | 14.07% |
| Risk 13 | 0.00% | 1.17% | 1.23% | 0.47% | 0.53% | 0.00% | 0.00% | 0.68% | 0.00% |
| Risk 14 | 7.11% | 8.17% | 4.12% | 2.79% | 3.16% | 3.09% | 1.69% | 2.04% | 0.00% |
| Risk 15 | 30.46% | 19.46% | 20.58% | 18.14% | 15.79% | 11.11% | 13.56% | 12.24% | 5.93% |
| Risk 16 | 27.92% | 26.46% | 32.92% | 33.95% | 35.26% | 33.95% | 36.72% | 33.33% | 40.00% |
| Risk 17 | 1.02% | 0.00% | 0.00% | 0.47% | 0.53% | 0.00% | 0.56% | 0.00% | 0.74% |
| Risk 18 | 2.03% | 2.33% | 0.82% | 0.00% | 2.63% | 1.23% | 0.56% | 0.00% | 0.74% |
| Risk 19 | 0.00% | 0.39% | 0.00% | 0.47% | 0.00% | 0.00% | 0.00% | 0.00% | 0.00% |

Since January 2012 the top high risk construction category has been 16 - *Construction work on construction-sites where there is any movement of powered mobile plant*. The increased occurrence of incidents in this category could be attributed to the prevalence of mobile plant on most construction sites. Mobile Plant continues to be one of the main hazards reviewed at audit.

There is consistently a significant difference between the first and second highest rated risk, with an average difference of 13.83 per cent. With the exception of the January to June 2013 reporting period, the second highest rating category has alternated between 1 - *Construction work with risk of a person falling two metres or more* and 15 - *Construction work on or adjacent to roadways or railways used by road or rail traffic.*

Risk 15 - *Construction work on or adjacent to roadways or railways used by road or rail traffic* recorded a sizeable decrease (56.27 per cent) from 13.56 per cent in the corresponding period in 2014 to 5.93 per cent in the current period. Risk 16 recorded the highest number of incidents (33.33 per cent) since the OFSC began collecting this information in the July to December 2011 reporting period, with an 8.93 per cent increase from the corresponding period in 2014.

## 

## 4.5 Working Time Lost

There has been no change in the most common length of working time lost since the OFSC began collecting this information in July to December 2011. B*etween one and three days* remains the highest ranking category, followed by *one week to less than two weeks.* There is consistently a significant percentage difference between the first and second highest categories (average 21.00 per cent)

There was a significant decrease to the proportion of injuries resulting in *three days to less than one week* of working time lost (14.15 per cent compared to 21.75 per cent in the corresponding period in 2014). Over 73 per cent of workers who suffered a lost time injury returned to work in less than two weeks.

**Working Time Lost**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Period | A | B | C | D | E | F |
| Jul to Dec 2011 | 45.26% | 22.40% | 13.98% | 9.47% | 7.22% | 1.65% |
| Jan to Jun 2012 | 46.41% | 17.66% | 13.55% | 12.53% | 8.21% | 1.64% |
| Jul to Dec 2012 | 34.79% | 25.00% | 13.75% | 13.33% | 9.58% | 3.54% |
| Jan to Jun 2013 | 46.67% | 23.20% | 12.27% | 8.80% | 6.67% | 2.40% |
| Jul to Dec 2013 | 38.67% | 20.82% | 17.85% | 13.73% | 7.09% | 1.83% |
| Jan to Jun 2014 | 41.71% | 22.61% | 15.83% | 11.31% | 7.79% | 0.75% |
| Jul to Dec 2014 | 42.75% | 21.75% | 12.25% | 13.75% | 7.00% | 2.50% |
| Jan to Jun 2015 | 41.71% | 21.14% | 16.29% | 12.29% | 6.57% | 2.00% |
| Jul to Dec 2015 | 40.57% | 14.15% | 18.55% | 14.78% | 7.86% | 4.09% |

## 4.6 Age Breakdown

Over 72 per cent of injured workers were below the age of 45. The 25-34 age bracket continues to account for the highest number of reported incidents (37.74 per cent).

**Incident Age Breakdown**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Period | 15-24 | 25-34 | 35-44 | 45-54 | 55-64 | 65 & Over |
| Jul to Dec 2011 | 19.77% | 28.65% | 21.97% | 19.96% | 8.69% | 0.96% |
| Jan to Jun 2012 | 20.77% | 28.18% | 22.13% | 20.02% | 7.66% | 1.24% |
| Jul to Dec 2012 | 17.84% | 33.24% | 25.00% | 15.14% | 7.43% | 1.35% |
| Jan to Jun 2013 | 18.20% | 33.33% | 20.93% | 16.59% | 9.66% | 1.29% |
| Jul to Dec 2013 | 19.55% | 34.62% | 23.24% | 13.30% | 8.65% | 0.64% |
| Jan to Jun 2014 | 19.48% | 31.84% | 25.47% | 16.48% | 5.99% | 0.75% |
| Jul to Dec 2014 | 19.05% | 30.67% | 20.38% | 18.86% | 9.14% | 1.90% |
| Jan to Jun 2015 | 16.99% | 35.46% | 23.14% | 15.50% | 8.28% | 0.64% |
| Jul to Dec 2015 | 12.50% | 37.74% | 21.88% | 17.07% | 10.58% | 0.24% |

## 4.7 Injured Person’s Occupation

Over 92 per cent of people injured in reports submitted to the OFSC were Tradesmen (54.18 per cent) or Labourers (38.19 per cent).

**Workers Occupation**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Period | 1 | 2 | 3 | 4 | 5 | 6 | 7 |
| Jul to Dec 2011 | 42.22% | 47.47% | 1.15% | 1.43% | 1.72% | 0.19% | 5.83% |
| Jan to Jun 2012 | 45.49% | 44.99% | 2.10% | 1.11% | 1.48% | 0.37% | 4.45% |
| Jul to Dec 2012 | 41.37% | 48.92% | 2.02% | 0.54% | 2.16% | 0.13% | 4.85% |
| Jan to Jun 2013 | 42.58% | 47.69% | 1.91% | 0.48% | 1.91% | 0.00% | 5.42% |
| Jul to Dec 2013 | 37.85% | 49.84% | 2.34% | 0.93% | 2.18% | 0.31% | 6.54% |
| Jan to Jun 2014 | 41.65% | 47.28% | 1.05% | 1.05% | 2.11% | 0.53% | 6.33% |
| Jul to Dec 2014 | 40.59% | 48.89% | 1.48% | 1.29% | 1.48% | 0.18% | 6.09% |
| Jan to Jun 2015 | 47.40% | 42.62% | 0.83% | 1.66% | 1.87% | 0.00% | 5.61% |
| Jul to Dec 2015 | 38.19% | 54.18% | 1.43% | 1.91% | 1.91% | 0.24% | 2.15% |

## 4.8 Dangerous Occurrences

The OFSC encourages companies to accurately report Dangerous Occurrences both internally and to external bodies such as the OFSC. A Dangerous Occurrence (or ‘near miss’) can be as revealing of WHS system inadequacies as an incident that *does* result in an injury or fatality.

Forty-six Scheme Dangerous Occurrences were reported to the OFSC in the July to December 2015 reporting period. This is the lowest number reported since the OFSC began collecting this data in 2011.

There was again some correlation between the circumstances of the Dangerous Occurrences reported to the OFSC and those of the incidents resulting in injury. The most common high-risk work nominated in Dangerous Occurrence incident reports was also the most commonly nominated in LTI/MTI/Fatality reports (work on construction sites where there is any movement of powered mobile plant).

**Dangerous Occurrences**

|  |  |
| --- | --- |
| Period | Dangerous Occurrences |
| Jul to Dec 2011 | 79 |
| Jan to Jun 2012 | 89 |
| Jul to Dec 2012 | 83 |
| Jan to Jun 2013 | 84 |
| Jul to Dec 2013 | 76 |
| Jan to Jun 2014 | 53 |
| Jul to Dec 2014 | 49 |
| Jan to Jun 2015 | 58 |
| Jul to Dec 2015 | 46 |

## 4.9 Workers’ Compensation

Accredited contractors continue to be well below the industry average for Workers Compensation Premium Rates (approximately 34 per cent1).

**Accredited Contractors**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Period | Mean premium rate ACT % | Mean premium rate NSW % | Mean premium rate NT % | Mean premium rate QLD % | Mean premium rate SA % | Mean premium rate TAS % | Mean premium rate VIC % | Mean premium rate WA % |
| Jul to Dec 2007 | 5.589 | 3.069 | 2.675 | 1.346 | 2.940 | . | 3.098 | 2.496 |
| Jan to Jun 2008 | 4.962 | 3.508 | 2.355 | 1.438 | 3.037 | . | 2.054 | 3.348 |
| Jul to Dec 2008 | 4.274 | 3.106 | 2.261 | 1.568 | 3.750 | 1.087 | 2.297 | 2.066 |
| Jan to Jun 2009 | 3.742 | 2.811 | 1.973 | 1.117 | 3.832 | 1.155 | 2.289 | 2.342 |
| Jul to Dec 2009 | 3.849 | 3.351 | 2.376 | 1.424 | 3.695 | 1.302 | 2.202 | 1.948 |
| Jan to Jun 2010 | 3.521 | 2.975 | 2.372 | 1.316 | 3.560 | 1.475 | 2.270 | 1.731 |
| Jul to Dec 2010 | 3.025 | 3.051 | 2.389 | 1.548 | 3.845 | 1.015 | 1.980 | 1.896 |
| Jan to Jun 2011 | 3.699 | 3.014 | 2.310 | 1.449 | 3.668 | 1.701 | 1.905 | 1.767 |
| Jul to Dec 2011 | 3.534 | 3.019 | 2.028 | 1.735 | 2.913 | 2.277 | 1.746 | 1.518 |
| Jan to Jun 2012 | 3.712 | 3.102 | 3.508 | 1.717 | 3.204 | 2.014 | 1.680 | 3.048 |
| Jul to Dec 2012 | 3.488 | 3.177 | 2.303 | 1.702 | 2.981 | 1.858 | 1.773 | 1.568 |
| Jan to Jun 2013 | 3.442 | 3.217 | 2.324 | 1.769 | 2.801 | 1.935 | 1.584 | 1.627 |
| Jul to Dec 2013 | 3.318 | 2.906 | 2.334 | 1.728 | 2.705 | 2.275 | 1.531 | 1.466 |
| Jan to Jun 2014 | 3.750 | 2.851 | 2.125 | 1.713 | 2.805 | 2.234 | 1.524 | 1.533 |
| Jul to Dec 2014 | 3.303 | 2.529 | 1.913 | 1.558 | 2.749 | 2.126 | 1.490 | 1.471 |
| Jan to Jun 2015 | 3.020 | 2.461 | 2.046 | 1.423 | 2.517 | 1.938 | 1.461 | 1.359 |
| Jul to Dec 2015 | 3.162 | 2.507 | 2.115 | 1.447 | 2.523 | 2.095 | 1.465 | 1.370 |

**Industry**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Period | Mean premium rate ACT % | Mean premium rate NSW % | Mean premium rate NT % | Mean premium rate QLD % | Mean premium rate SA % | Mean premium rate TAS % | Mean premium rate VIC % | Mean premium rate WA % |
| House construction September 2014[[2]](#footnote-2)1 | NA | 3.666 | NA | 2.437 | 3.19 | 4.23 | 1.736 | 1.11 |
| Non-residential construction September 20141 | NA | 2.858 | NA | 2.33 | 3.08 | 3.58 | 1.625 | 2.02 |

## 5 Awards and Recognition

During this reporting period accredited contractors have been the recipients of a number of prestigious safety awards, including—but not limited to—the following:

* Decmil Australia Pty Ltd – won the 2015 Queensland WorkSafe Award for ‘Best Work Health and Safety Management System’

* Shape Australia Pty Ltd – won the 2015 Master Builders Association of NSW award for ‘Site Safety – Commercial Projects up to $50,000,000’
* Shaw Contracting Pty Ltd – won the Civil Contractors Federation TAS 2015 Earth Award for ‘Safety at Roadworks’
* Watpac Construction Pty Ltd – won the ‘Office of the Federal Safety Commissioner National Excellence in Workplace Health and Safety’ award at Master Builders National Awards.

## 6 Initiatives


Accredited contractors submit details of any safety initiatives developed by their company during the reporting period. Many of these initiatives will form the basis of case studies and fact sheets to be published on fsc.gov.au over the coming months.

## Glossary


**Arithmetic mean (average)** - The mean is the sum of all the scores divided by the number of scores.

**Dangerous occurrence** - An incident where no person is injured, but could have been injured, resulting in Serious Personal Injury, Incapacity or Death. Also commonly called a “near miss”.

**Fatality Frequency Rate** – Fatality Frequency rates are calculated as follows:



**Frequency rate** - Frequency rates are calculated as follows:



**High-risk construction work hazards**

1. Construction work where there is a risk of a person falling two metres or more
2. Construction work on telecommunications towers
3. Construction work involving demolition
4. Construction work involving the disturbance or removal of asbestos
5. Construction work involving structural alterations that require temporary support to prevent collapse
6. Construction work involving a confined space
7. Construction work involving excavation to a depth greater than 1.5 metres
8. The construction of tunnels
9. Construction work involving the use of explosives
10. Construction work on or near pressurised gas distribution mains and consumer piping
11. Construction work on or near chemical, fuel or refrigerant lines
12. Construction work on or near energised electrical installations and services
13. Construction work in an area that may have a contaminated or flammable atmosphere
14. Tilt-up and precast concrete construction work
15. Construction work on or adjacent to roadways or railways used by road or rail traffic
16. Work on construction sites where there is any movement of powered mobile plant
17. Construction work in an area where there are artificial extremes of temperature
18. Construction work in, over or adjacent to water or other liquids where there is a risk of drowning
19. Construction work involving diving

**Incident** - An incident resulting in an injury that is required to be notified by the WHS legislative requirement for notifiable incidents in the jurisdiction in which the project is being undertaken.

**LTIFR (Lost Time Injury Frequency Rate)** - The number of occurrences of lost time injury that result in a fatality, a permanent disability or time lost from work of one day shift or more in the period. The number of hours worked refers to the total number of hours worked by all workers in the period, including overtime and extra shifts.

**Mechanism of incident classification**

Major Groups

0. Falls, trips and slips of a person

1. Hitting objects with a part of the body

2. Being hit by moving objects

3. Sound and pressure

4. Body stressing

5. Heat, electricity and other environmental factors

6. Chemicals and other substances

7. Biological factors

8. Mental stress

9. Vehicle incidents and other

**Median** - The median is the middle of a distribution; half the scores are above the median and half are below the median. If the number of values in the data set is even, then the median is the average of the two middle values. The median is less sensitive to extreme scores than the average.

**MTIFR (Medically Treated Injury Frequency Rate)** - The number of occurrences of treatment by, or under the order of, a qualified medical practitioner, or any injury that could be considered as being one that would normally be treated by a medical practitioner. The number of hours worked refers to the total number of hours worked by all workers in the period, including overtime and extra shifts.

**Nature of injury classification**

1. Intracranial injuries
2. Fractures
3. Wounds, lacerations, amputations and internal organ damage
4. Burns
5. Injury to nerves and spinal cord
6. Traumatic joint/ligament and muscle/tendon injury
7. Other injuries
8. Diseases and conditions

**Non-Scheme projects** – Projects where the accredited contractor is the head contractor, the value of building work is $3 million or more, and the project is not a Scheme project.

**Scheme projects** - Projects that are directly funded by the Australian Government with a value of $3 million or more, plus, projects that are indirectly funded by the Australian Government where:

* the value of the Australian Government contribution to the project is at least $5 million and represents at least 50 per cent of the total construction project value; or
* the Australian Government contribution to a project is $10 million or more, irrespective of the proportion of Australian Government funding.

**TRIFR (Total Recorded Injury Frequency Rate)** – The total number of Medically Treated Injuries, Lost Time Injuries and Fatalities in the defined period divided by the number of hours worked in the period, multiplied by one million.

**Winsorised mean** - involves the calculation of the mean after replacing given parts of a distribution at the high and low end with the most extreme remaining values, typically replacing an equal amount of both ends. Often 10 per cent of the ends are replaced. The winsorised mean is a useful estimator because it is less sensitive to outliers than the mean but will still give a reasonable estimate of central tendency.

1. 331 accreditations representing 390 companies. [↑](#footnote-ref-1)
2. 1 *Source:* Safe Work Australia publication Comparison of Workers’ Compensation Arrangements in Australia and New Zealand July 2015, Table 7.6 Selected Industry Premium Rates as at 30 September 2014, pages 199-202. [↑](#footnote-ref-2)