**Hazard 2020: Oct 2020 – June 2021 Update**



|  |
| --- |
| **Hazard 2020 Audits** |
| Completed | **211** |
| In Progress  | **67** |
| **Total** | **278** |

**Most frequently issued CAR sub-criteria on Hazard 2020 Audits**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Mobile Plant** | **CARs Issued** | **Times audited** | **CAR Issue Rate** | **Compared to trend\*** |
| **H16.3:** Safe systems of work are established for the operation of mobile plant taking into account; the operator manual, outcomes from the plant risk assessment, site specific requirements & the need for ROPS & FOPS. | **72** | **192** | **37.5%** | **-6.0%** |
| **H16.5:** Safe systems developed for mobile cranes taking into account ground conditions; development of lift plans in accordance with relevant legislation, codes of practice, Australian standards; & lifting of materials & workers. | **66** | **192** | **34.4%** | **+0.2%** |
| **H16.9: S**ystem ensures an inspection program specific to the needs of type of plant, taking into account regulatory inspections/registration; manufacturers’ inspection requirements; pre-start inspections; & commissioning. | **66** | **192** | **34.4%** | **-4.0%** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Scaffolding** | **CARs Issued** | **Times audited** | **CAR Issue Rate** | **Compared to trend\*** |
| **H5.6:** System ensures structural support systems & temporary structures are installed by a competent person, verified as correctly installed prior to use in accordance with legislation, codes of practice & Australian standards; manufacturers’ requirements; or where applicable the drawing/plan. | **32** | **60** | **53.3%** | **+11.3%** |
| **H1.4:** Safe systems of work have been developed to ensure that where fall restraint/fall arrest equipment is being used onsite: workers have been formally trained in the use of equipment; there is a maintenance & inspection schedule for the equipment; attachment points are designed & certified by a qualified person; attachment points are installed by a trained person & regularly inspected by a competent person. | **32** | **75** | **42.7%** | **-1.2%** |
| **H5.4:** The system ensures scaffold plan developed by a qualified person; & changes to installation design are authorised & signed off by a qualified person; or risk assessment conducted to determine need for a Scaffold Plan. | **28** | **60** | **46.7%** | **-0.2%** |

**All data is from 16 October 2020 – 28 June 2021. For more information see** [**www.fsc.gov.au**](http://www.fsc.gov.au)

**\*CAR issue comparison rates are from all Scheme audits 2017-2019**